Control Freak SE Profiles for Line6 Pod

NOTES:

L6POD__1.MID
L6POD__2.MID
L6POD__3.MID

Name | LNE6EQ/AMP/VL/FX
File | L6POD__1.MID | Location | 63
Slider 1: | AMP MODEL | Button 1: | On | BRIGHT SWTCH ON | Off | BRIGHT SWTCH OFF
Slider 2: | DRIVE | Button 2: | On | DISTORTION ON | Off | DISTORTION OFF
Slider 3: | DRIVE 2 | Button 3: | On | DRIVE/BOOST ON | Off | DRIVE/BOOST OFF
Slider 4: | BASS | Button 4: | On | EQ ON | Off | EQ OFF
Slider 5: | MID | Button 5: | On |  | Off |
Slider 6: | TREBLE | Button 6: | On |  | Off |
Slider 7: | PRESENCE | Button 7: | On |  | Off |
Slider 8: | CHANNEL VOLUME | Button 8: | On |  | Off |
Slider 9: | GATE THRESHOLD | Button 9: | On | NOISE GATE ON | Off | NOISE GATE OFF
Slider 10: | GATE DECAY | Button 10: | On |  | Off |
Slider 11: | FX SELECT | Button 11: | On |  | Off |
Slider 12: | FX TWEAK | Button 12: | On |  | Off |
Slider 13: | VOLUME PEDAL | Button 13: | On | VOL PDL PRE TUBE | Off | VOL PDL PST TUBE
Slider 14: | VOL SWELL RAMP | Button 14: | On | VOLUME SWELL ON | Off | VOLUME SWELL OFF
Slider 15: | VOLUME PEDAL MIN | Button 15: | On |  | Off |
Slider 16: | CABINET TYPE | Button 16: | On |  | Off |

top..

Name | LNE6 PD DLY/VERB
File | L6POD__2.MID | Location | 63
Slider 1: | DELAY TIME 1 | Button 1: | On | DELAY ON | Off | DELAY OFF
Slider 2: | DELAY TIME 1 x2 | Button 2: | On | DELAY MONO | Off | DELAY STEREO
Slider 3: | DELAY TIME 2 | Button 3: | On |  | Off |
Slider 4: | DELAY TIME 2 x2 | Button 4: | On |  | Off |
Slider 5: | DELAY REGEN 1 | Button 5: | On |  | Off |
Slider 6: | DELAY REGEN 2 | Button 6: | On |  | Off |
Slider 7: | DELAY LEVEL 1 | Button 7: | On |  | Off |
Slider 8: | DELAY LEVEL 2 | Button 8: | On | TAP TEMPO | Off |
Slider 9: | REVERB DECAY | Button 9: | On | REVERB ON | Off | REVERB OFF
Slider 10: | REVERB TONE | Button 10: | On | REVERB HALL | Off | REVERB SPRING
Slider 11: | REVERB DIFFUSION | Button 11: | On |  | Off |
Slider 12: | REVERB DENSITY | Button 12: | On |  | Off |
Slider 13: | REVERB LEVEL | Button 13: | On |  | Off |
Slider 14: | WAH PEDAL | Button 14: | On | WAH PEDAL ON | Off | WAH PEDAL OFF
Slider 15: | WAH BOTTOM FREQ | Button 15: | On |  | Off |
Slider 16: | WAH TOP FREQ | Button 16: | On |  | Off |

top..

Name | LNE6 PD MDFX/RFX
File | L6POD__3.MID | Location | 63
Slider 1: | CHOR/FLANG SPEED | Button 1: | On | CHOR/ROTA/TREM.1 | Off | CHOR/ROTA/TREM.0
Slider 2: | CHOR/FLANG DEPTH | Button 2: | On | REGENERATION POS | Off | REGENERATION NEG
Slider 3: | CHORUS PREDELAY | Button 3: | On |  | Off |
Slider 4: | ROTARY SPEED | Button 4: | On |  | Off |
Slider 5: | ROTARY MIN/MAX | Button 5: | On |  | Off |
Slider 6: | TREMOLO SPEED | Button 6: | On |  | Off |
Slider 7: | TREMOLO DEPTH | Button 7: | On |  | Off |
Slider 8: | A.I.R AMBI LEVEL | Button 8: | On |  | Off |
Slider 9: |  | Button 9: | On | ROOMS/HALLS | Off |
Slider 10: |  | Button 10: | On | PLATES | Off |
Slider 11: |  | Button 11: | On | CHORUS/FLANGE | Off |
Slider 12: |  | Button 12: | On | DELAY 4 TAP | Off |
Slider 13: |  | Button 13: | On | CHORUS/RESONATOR | Off |
Slider 14: |  | Button 14: | On | INVERSE | Off |
Slider 15: |  | Button 15: | On | GATE | Off |
Slider 16: |  | Button 16: | On | DELAY | Off |

top..