Control Freak SE Profiles for Siel EX-80

NOTES:
SIEL EX-80 - created by Dennis Verhaeg Not tested by Kenton These should also work with DK-80

EX80_DCO.mid
EX80_VCA.mid
EX80_VCF.mid

Name | Siel EX-80 DCO
File | EX80_DCO.mid | Location | 63
Slider 1: | DCO off/squa/saw | Button 1: | On |  | Off |
Slider 2: | Saw 16'/8'/4' | Button 2: | On | LFO1 Delay Auto | Off | LFO1 Delay Man.
Slider 3: | Square level 16' | Button 3: | On |  | Off |
Slider 4: | Square level 8' | Button 4: | On |  | Off |
Slider 5: | Square level 4' | Button 5: | On | DCO Mode: Double | Off | DCO Mode: Whole
Slider 6: | Square level 2' | Button 6: | On | Noise Dest. VCF | Off | Noise Dest. VCA
Slider 7: | Noise level | Button 7: | On |  | Off |
Slider 8: |  | Button 8: | On |  | Off |
Slider 9: | LFO1 Delay | Button 9: | On |  | Off |
Slider 10: | LFO1 to DCO freq | Button 10: | On |  | Off |
Slider 11: | LFO1 Final Level | Button 11: | On |  | Off |
Slider 12: | LFO1 Initial lvl | Button 12: | On |  | Off |
Slider 13: | LFO1 Delay time | Button 13: | On |  | Off |
Slider 14: |  | Button 14: | On |  | Off |
Slider 15: |  | Button 15: | On |  | Off |
Slider 16: | Output Volume | Button 16: | On |  | Off |

top..

Name | Siel EX-80 VCA
File | EX80_VCA.mid | Location | 63
Slider 1: | VCA A Attack | Button 1: | On | VCA A Velocity | Off | VCA A NoVelocity
Slider 2: | VCA A Decay | Button 2: | On | DampingPedal on | Off | DampingPedal off
Slider 3: | VCA A Breakpoint | Button 3: | On | VCA B Velocity | Off | VCA B NoVelocity
Slider 4: | VCA A Slope | Button 4: | On | DampingPedal on | Off | DampingPedal off
Slider 5: | VCA A Sustain | Button 5: | On | DCO Mode: Double | Off | DCO Mode: Whole
Slider 6: | VCA A Release | Button 6: | On | Noise Dest. VCF | Off | Noise Dest. VCA
Slider 7: | Detune Interval | Button 7: | On |  | Off |
Slider 8: | Detune Fine | Button 8: | On |  | Off |
Slider 9: | VCA B Attack | Button 9: | On | Mute Chan 9 | Off | Reset Chan 9
Slider 10: | VCA B Decay | Button 10: | On | Mute Chan 10 | Off | Reset Chan 10
Slider 11: | VCA B Breakpoint | Button 11: | On | Mute Chan 11 | Off | Reset Chan 11
Slider 12: | VCA B Slope | Button 12: | On | Mute Chan 12 | Off | Reset Chan 12
Slider 13: | VCA B Sustain | Button 13: | On | Mute Chan 13 | Off | Reset Chan 13
Slider 14: | VCA B Release | Button 14: | On | Mute Chan 14 | Off | Reset Chan 14
Slider 15: | Noise Level | Button 15: | On | Mute Chan 15 | Off | Reset Chan 15
Slider 16: | Output Volume | Button 16: | On | Mute Chan 16 | Off | Reset Chan 16

top..

Name | Siel EX-80 VCF
File | EX80_VCF.mid | Location | 63
Slider 1: | VCF Attack | Button 1: | On | VCF Velocity on | Off | VCF Velocity off
Slider 2: | VCF Decay | Button 2: | On | LFO2 Delay Auto | Off | LFO2 Delay Man.
Slider 3: | VCF Breakpoint | Button 3: | On | LFO2 Wave Square | Off | LFO2 Wave Sawtoo
Slider 4: | VCF Slope | Button 4: | On | VCF trig. Multi | Off | VCF trig. Single
Slider 5: | VCF Sustain | Button 5: | On |  | Off |
Slider 6: | VCF Release | Button 6: | On |  | Off |
Slider 7: | VCF Cut off | Button 7: | On |  | Off |
Slider 8: | VCF Resonance | Button 8: | On |  | Off |
Slider 9: | VCF Env level | Button 9: | On |  | Off |
Slider 10: | LFO2 to VCF Freq | Button 10: | On |  | Off |
Slider 11: | LFO2 Final level | Button 11: | On |  | Off |
Slider 12: | LFO2 Initial lvl | Button 12: | On |  | Off |
Slider 13: | LFO2 Delay time | Button 13: | On |  | Off |
Slider 14: | VCF KbdTrack OHF | Button 14: | On |  | Off |
Slider 15: |  | Button 15: | On |  | Off |
Slider 16: | Output Volume | Button 16: | On |  | Off |

top..