Control Freak SE Profiles for Yamaha DX100

NOTES:

Dx100vce.mid

Name | DX100 VOICE
File | Dx100vce.mid | Location | 63
Slider 1: | ALGORITHMS 1 - 8 | Button 1: | On | MONO | Off | POLY
Slider 2: | FEEDBACK OP4 | Button 2: | On | SUSTAIN ON | Off | SUSTAIN OFF
Slider 3: | VOLUME OP1 | Button 3: | On | OP1 OFF | Off | OP1 ON
Slider 4: | VOLUME OP2 | Button 4: | On | OP2 OFF | Off | OP2 ON
Slider 5: | VOLUME OP3 | Button 5: | On | OP3 OFF | Off | OP3 ON
Slider 6: | VOLUME OP4 | Button 6: | On | OP4 OFF | Off | OP4 ON
Slider 7: | PORTA TIME | Button 7: | On | PORTA FINGERED | Off | PORTA FULLTIME
Slider 8: |  | Button 8: | On | PORTA ON | Off | PORTA OFF
Slider 9: | LFO DEPTH | Button 9: | On | LFO TRI WAVE | Off | LFO SQR WAVE
Slider 10: | VCF CUTOFF | Button 10: | On | VCF LFO ON | Off | VCF LFO OFF
Slider 11: | RESONANCE | Button 11: | On | OSC LFO ON | Off | OSC LFO OFF
Slider 12: | VCF ADSR DEPTH | Button 12: | On | VCF KEYTRACK 1/2 | Off | VCF KEYTRACK FUL
Slider 13: | VCF ADSR DECAY | Button 13: | On | PWM LFO ON | Off | PWM LFO OFF
Slider 14: | PORTAMENTO RATE | Button 14: | On | SAW WAVE ON | Off | SAW WAVE OFF
Slider 15: | AMP ADSR DECAY | Button 15: | On | SQR WAVE ON | Off | SQR WAVE OFF
Slider 16: | PULSEWIDTH | Button 16: | On | PWM LFO ON | Off | PWM LFO OFF

top..