Control Freak SE Profiles for Roland RD110

NOTES:

RD110__1.MID
RD110__2.MID
RD110__3.MID
RD110__4.MID

Name | RLND D110 WV/MOD
File | RD110__1.MID | Location | 63
Slider 1: | PITCH COARSE | Button 1: | On | P BEND ON | Off | P BEND OFF
Slider 2: | PITCH FINE | Button 2: | On |  | Off |
Slider 3: | PITCH KEYFOLLOW | Button 3: | On |  | Off |
Slider 4: | SQU/SAW PCM 1/2 | Button 4: | On |  | Off |
Slider 5: | PCM WAVE | Button 5: | On |  | Off |
Slider 6: | PULSEWIDTH | Button 6: | On |  | Off |
Slider 7: | PLSEWDTH V SENS | Button 7: | On |  | Off |
Slider 8: | ENV MODE | Button 8: | On |  | Off |
Slider 9: | PITCH LFO RATE | Button 9: | On |  | Off |
Slider 10: | PITCH LFO DEPTH | Button 10: | On |  | Off |
Slider 11: | PTCH LFO MODSENS | Button 11: | On |  | Off |
Slider 12: | PITCH ENV DEPTH | Button 12: | On |  | Off |
Slider 13: | PTCH ENV VELSENS | Button 13: | On |  | Off |
Slider 14: | PTCH ENV TIME KF | Button 14: | On |  | Off |
Slider 15: |  | Button 15: | On |  | Off |
Slider 16: |  | Button 16: | On |  | Off |

top..

Name | ROLAND D110 DCF
File | RD110__2.MID | Location | 63
Slider 1: | TVF CUTOFF | Button 1: | On |  | Off |
Slider 2: | TVF RESONANCE | Button 2: | On |  | Off |
Slider 3: | TVF KEYFOLLOW | Button 3: | On |  | Off |
Slider 4: | TVF BIAS POINT | Button 4: | On |  | Off |
Slider 5: | TVF BIAS LEVEL | Button 5: | On |  | Off |
Slider 6: | TVF ENV DEPTH | Button 6: | On |  | Off |
Slider 7: | TVF ENV VEL SENS | Button 7: | On |  | Off |
Slider 8: | TVF ENV DEPTH KF | Button 8: | On |  | Off |
Slider 9: | TVF ENV TIME KF | Button 9: | On |  | Off |
Slider 10: | TVF ENV TIME 1 | Button 10: | On |  | Off |
Slider 11: | TVF ENV TIME 2 | Button 11: | On |  | Off |
Slider 12: | TVF ENV TIME 3 | Button 12: | On |  | Off |
Slider 13: | TVF ENV TIME 4 | Button 13: | On |  | Off |
Slider 14: | TVF ENV LEVEL 1 | Button 14: | On |  | Off |
Slider 15: | TVF ENV LEVEL 2 | Button 15: | On |  | Off |
Slider 16: | TVF ENV LEVEL 3+ | Button 16: | On |  | Off |

top..

Name | ROLAND D110 DCA
File | RD110__3.MID | Location | 63
Slider 1: | TVA LEVEL | Button 1: | On |  | Off |
Slider 2: | TVA VEL SENS | Button 2: | On |  | Off |
Slider 3: | TVA BIAS POINT 1 | Button 3: | On |  | Off |
Slider 4: | TVA BIAS LEVEL 1 | Button 4: | On |  | Off |
Slider 5: | TVA BIAS POINT 2 | Button 5: | On |  | Off |
Slider 6: | TVA BIAS LEVEL 2 | Button 6: | On |  | Off |
Slider 7: | TVA ENV TIME VF | Button 7: | On |  | Off |
Slider 8: | MIDI VOLUME cc7 | Button 8: | On |  | Off |
Slider 9: | TVA ENV TIME KF | Button 9: | On |  | Off |
Slider 10: | TVA ENV TIME 1 | Button 10: | On |  | Off |
Slider 11: | TVA ENV TIME 2 | Button 11: | On |  | Off |
Slider 12: | TVA ENV TIME 3 | Button 12: | On |  | Off |
Slider 13: | TVA ENV TIME 4 | Button 13: | On |  | Off |
Slider 14: | TVA ENV LEVEL 1 | Button 14: | On |  | Off |
Slider 15: | TVA ENV LEVEL 2 | Button 15: | On |  | Off |
Slider 16: | TVA ENV LEVEL 3+ | Button 16: | On |  | Off |

top..

Name | RLND D110 VRB/LV
File | RD110__4.MID | Location | 63
Slider 1: | REVERB MODE | Button 1: | On |  | Off |
Slider 2: | REVERB TIME | Button 2: | On |  | Off |
Slider 3: | REVERB LEVEL | Button 3: | On |  | Off |
Slider 4: | UPPER REV SWITCH | Button 4: | On |  | Off |
Slider 5: | LOWER REV SWITCH | Button 5: | On |  | Off |
Slider 6: | REVERB SWITCH | Button 6: | On |  | Off |
Slider 7: | SPLIT POINT | Button 7: | On |  | Off |
Slider 8: | KEY MODE | Button 8: | On |  | Off |
Slider 9: | PCM WAVE | Button 9: | On | WAVEFORM SQU 1 | Off |
Slider 10: | PULSEWIDTH | Button 10: | On | WAVEFORM SAW 1 | Off |
Slider 11: | TVF CUTOFF | Button 11: | On | PCM BANK 1 | Off |
Slider 12: | TVF RESONANCE | Button 12: | On | PCM BANK 2 | Off |
Slider 13: | TVF KEYFOLLOW | Button 13: | On |  | Off |
Slider 14: | TVF ENV DEPTH | Button 14: | On |  | Off |
Slider 15: | STRUCTURE 1+2 | Button 15: | On |  | Off |
Slider 16: | STRUCTURE 3+4 | Button 16: | On | KEY OFF ACCEPT | Off | KEY OFF IGNORE

top..