Control Freak SE Profiles for Waldorf Pulse

NOTES:

PULSE__A.MID
PULSE__B.MID
PULSE__C.MID

Name | PULSE+ VCO 1/2
File | PULSE__A.MID | Location | 63
Slider 1: | OSC 1 SEMITONE | Button 1: | On | OSC 1 WAVE PULSE | Off |
Slider 2: | OSC 1 TUNE | Button 2: | On | OSC 1 WAVE SAW | Off |
Slider 3: | OSC 1 PULSEWIDTH | Button 3: | On | OSC 1 WAVE TRI | Off |
Slider 4: | OSC 2 SEMITONE | Button 4: | On | OSC 2 WAVE PULSE | Off |
Slider 5: | OSC 2 TUNE | Button 5: | On | OSC 2 WAVE SAW | Off |
Slider 6: | OSC 2 PULSEWIDTH | Button 6: | On | OSC 2 WAVE TRI | Off |
Slider 7: | OSC 2 KEYTRACK | Button 7: | On | OSC 2 CROSSMOD | Off |
Slider 8: | OSC 2 SYNC | Button 8: | On | OSC 2 SYNC ON | Off | OSC 2 SYNC OFF
Slider 9: | OSC 3 SEMITONE | Button 9: | On | OSC 3 WAVE PULSE | Off |
Slider 10: | OSC 3 TUNE | Button 10: | On | OSC 3 WAVE SAW | Off |
Slider 11: |  | Button 11: | On | OSC 3 WAVE TRI | Off |
Slider 12: | OSC 1 LEVEL | Button 12: | On |  | Off |
Slider 13: | OSC 2 LEVEL | Button 13: | On |  | Off |
Slider 14: | OSC 3 LEVEL | Button 14: | On |  | Off |
Slider 15: | NOISE LEVEL | Button 15: | On |  | Off |
Slider 16: | EXT INPUT LEVEL | Button 16: | On |  | Off |

top..

Name | PULSE+ LFOs/MOD
File | PULSE__B.MID | Location | 63
Slider 1: | LFO 1 SPEED | Button 1: | On | LFO 1 SINE | Off |
Slider 2: | LFO 2 SPEED | Button 2: | On | LFO 1 TRIANGLE | Off |
Slider 3: | LFO 2 DELAY | Button 3: | On | LFO 1 SAWTOOTH | Off |
Slider 4: | FILTA MOD SOURCE | Button 4: | On | LFO 1 PULSE | Off |
Slider 5: | FILTA MOD AMOUNT | Button 5: | On | LFO 1 SAMPLE+HLD | Off |
Slider 6: | PITCH MOD SOURCE | Button 6: | On | LFO 1 TRI SYNC | Off |
Slider 7: | PITCH MOD AMOUNT | Button 7: | On | LFO 1 SAW SYNC | Off |
Slider 8: | PITCHBEND SCALE | Button 8: | On | LFO 1 PULSE SYNC | Off |
Slider 9: | ARP OCTAVE RANGE | Button 9: | On | ARP ON | Off | ARP OFF
Slider 10: | ARP CLOCK | Button 10: | On | ARP HOLD | Off |
Slider 11: | ARP TEMPO | Button 11: | On | ARP UP | Off | ARP DOWN
Slider 12: | ENV 1 KEYTRACK | Button 12: | On | ARP PENDULUM | Off |
Slider 13: | ENV 2 KEYTRACK | Button 13: | On | ARP RANDOM | Off |
Slider 14: | CV2 MOD SOURCE | Button 14: | On | ARP ASSIGN UP | Off |
Slider 15: | CV2 MOD AMOUNT | Button 15: | On | ARP ASSIGN DOWN | Off |
Slider 16: | PORTAMENTO MODE | Button 16: | On | ARP ASSIGN PEND | Off |

top..

Name | PULSE+ VCF
File | PULSE__C.MID | Location | 63
Slider 1: | CUTOFF | Button 1: | On |  | Off |
Slider 2: | RESONANCE | Button 2: | On |  | Off |
Slider 3: | KEYTRACK | Button 3: | On |  | Off |
Slider 4: | ENV AMOUNT | Button 4: | On |  | Off |
Slider 5: | ENV 1 ATTACK | Button 5: | On | ENV 1 TRIGGER S1 | Off |
Slider 6: | ENV 1 DECAY | Button 6: | On | ENV 1 TRIGGER S2 | Off |
Slider 7: | ENV 1 SUSTAIN | Button 7: | On | ENV 1 TRIGGER R1 | Off |
Slider 8: | ENV 1 RELEASE | Button 8: | On | ENV 1 TRIGGER R2 | Off |
Slider 9: | VCA VOLUME | Button 9: | On |  | Off |
Slider 10: | VCA VEL SENS | Button 10: | On |  | Off |
Slider 11: | PANORAMA MOD | Button 11: | On |  | Off |
Slider 12: | MASTER VOLUME | Button 12: | On |  | Off |
Slider 13: | ENV 2 ATTACK | Button 13: | On | ENV 2 TRIGGER S1 | Off |
Slider 14: | ENV 2 DECAY | Button 14: | On | ENV 2 TRIGGER S2 | Off |
Slider 15: | ENV 2 SUSTAIN | Button 15: | On | ENV 2 TRIGGER R1 | Off |
Slider 16: | ENV 2 RELEASE | Button 16: | On | ENV 2 TRIGGER R2 | Off |

top..