Control Freak SE Profiles for Sequential Circuits 6Trak

NOTES:

6trak__a.mid
6trak__b.mid

Name | 6TRAK Osc/EG/Flt
File | 6trak__a.mid | Location | 63
Slider 1: | OSC COARSE TUNE | Button 1: | On | SAW WAVE ON | Off | SAW WAVE OFF
Slider 2: | OSC FINE TUNE | Button 2: | On | TRI WAVE ON | Off | TRI WAVE OFF
Slider 3: | PORTAMENTO RATE | Button 3: | On | SQR WAVE ON | Off | SQR WAVE OFF
Slider 4: | OSC ADSR DEPTH | Button 4: | On | OSC ADSR INVERT | Off | OSC ADSR NORMAL
Slider 5: | OSC ADSR ATTACK | Button 5: | On | OSC LFO ON | Off | OSC LFO OFF
Slider 6: | OSC ADSR DECAY | Button 6: | On | LFO TRI WAVE | Off |
Slider 7: | OSC ADSR RELEASE | Button 7: | On | LFO SQR WAVE | Off |
Slider 8: | PULSEWIDTH | Button 8: | On | PWM LFO ON | Off | PWM LFO OFF
Slider 9: | OSC / NOISE MIX | Button 9: | On | VCF KEYTRACK OFF | Off |
Slider 10: | VCF CUTOFF | Button 10: | On | VCF KEYTRACK 1/2 | Off |
Slider 11: | RESONANCE | Button 11: | On | VCF KEYTRACK FUL | Off |
Slider 12: | VCF ADSR DEPTH | Button 12: | On | VCF ADSR INVERT | Off | VCF ADSR NORMAL
Slider 13: | VCF ADSR ATTACK | Button 13: | On | VCF LFO ON | Off | VCF LFO OFF
Slider 14: | VCF ADSR DECAY | Button 14: | On | LFO TRI WAVE | Off |
Slider 15: | VCF ADSR RELEASE | Button 15: | On | LFO SQR WAVE | Off |
Slider 16: | TRIANGLE OSC MOD | Button 16: | On | UNISON ON | Off | UNISON OFF

top..

Name | 6TRAK LFO/VCA/Lv
File | 6trak__b.mid | Location | 63
Slider 1: | LFO SPEED | Button 1: | On |  | Off |
Slider 2: | LFO INITL AMOUNT | Button 2: | On |  | Off |
Slider 3: |  | Button 3: | On |  | Off |
Slider 4: | AMP ADSR ATTACK | Button 4: | On |  | Off |
Slider 5: | AMP ADSR DECAY | Button 5: | On |  | Off |
Slider 6: | AMP ADSR SUSTAIN | Button 6: | On |  | Off |
Slider 7: | AMP ADSR RELEASE | Button 7: | On | ENABLE ALL MIDI | Off |
Slider 8: | VOLUME | Button 8: | On | DOUBLE MODE | Off |
Slider 9: | LFO DEPTH | Button 9: | On | LFO TRI WAVE | Off | LFO SQR WAVE
Slider 10: | VCF CUTOFF | Button 10: | On | VCF LFO ON | Off | VCF LFO OFF
Slider 11: | RESONANCE | Button 11: | On | OSC LFO ON | Off | OSC LFO OFF
Slider 12: | VCF ADSR DEPTH | Button 12: | On | VCF KEYTRACK 1/2 | Off | VCF KEYTRACK FUL
Slider 13: | VCF ADSR DECAY | Button 13: | On | PWM LFO ON | Off | PWM LFO OFF
Slider 14: | PORTAMENTO RATE | Button 14: | On | SAW WAVE ON | Off | SAW WAVE OFF
Slider 15: | AMP ADSR DECAY | Button 15: | On | SQR WAVE ON | Off | SQR WAVE OFF
Slider 16: | PULSEWIDTH | Button 16: | On | PWM LFO ON | Off | PWM LFO OFF

top..